C

drawi.ino
Go to the documentation of this file.
1 /**----------------------------------------------------------------------------------*/
2 void drawRadio()
3 {
4 Serial.println(F(">>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>> "));
5 Serial.println(F("Attach radio directly to Arduino on pin 8 to gnd as shown below"));
6 Serial.println(F("or solder some wires so you can connect the radio on the shields"));
7 Serial.println(F("to 8,10,11,13 and 14. Remove any jumpers on shield "));
8 Serial.println(F(" "));
9 Serial.println(F(" ---------------"));
10 Serial.println(F(" | A aref"));
11 Serial.println(F(" | R GND-++-GND-------------"));
12 Serial.println(F(" | D 13 ++ 5V |=antenna =======>"));
13 Serial.println(F(" IOREF U 12 -- ENABLE(high) |"));
14 Serial.println(F(" RESET I 11 ++ RX |"));
15 Serial.println(F(" 3.3V N 10 ++ TX |"));
16 Serial.println(F(" 5V O 09 -- not used |"));
17 Serial.println(F(" GND 08-++ CONFIG(low)----|"));
18 Serial.println(F(" GND P |"));
19 Serial.println(F(" | B ~ 06"));
20 Serial.println(F(" A0 ~ 05"));
21 Serial.println(F(" A1 04"));
22 Serial.println(F(" A2 ~ 03"));
23 Serial.println(F(" A3 02"));
24 Serial.println(F(" A4 TX 01"));
25 Serial.println(F(" A5 RX 00"));
26 Serial.println(F(" ---------------"));
27 }
28
drawRadio
void drawRadio()
Definition: drawi.ino:2